**Large Gauge**

* RED → AC Lead 1
* BLACK → AC Lead 2
* GREEN/YELLOW → Earth Ground

**Small Gauge**

* PURPLE → Control Pilot → OpenEVSE Controller Pilot [PLT] connector
* BLUE → Charge port transmitter → 3.3v output of the WiFi Controller (To use an OpenEVSE 5v output add a few diodes in series to drop the voltage down a bit)
* BLACK → not used
* ORANGE → not used
* WHITE → not used